[Installation]
Product=MC Series Driver
Configuration=ZSU_AstroMCSeries.DLL
Driver=ZSD_AstroMCSeries.DLL
UI=ZSU_AstroMCSeries.DLL

[Units]
MarginPerInch=600
MarginPerCM=254     ; 300/2.54
ExtentPerInch=100

[DefaultPrinter]
DefaultFeed=1
;; Sets the print quality of the bitonal later
;;BitonalPrintQuality=800
PrintQuality=800
;; Set these values if additional resolutions are to be added
Resolution=800
;ResolutionXY=800,800, 1600,1600
;; These values specify the resolution the printer is capable
;; of printing at. By contrast, the PrintQuality value is what
;; we render at.
PhysicalResolutionX=1600
PhysicalResolutionY=1600
Capabilities=1,2,3,4,7,9,10,11,12,16
Formats=0,1,2,3,4,5,6
Bins=7,4
Source=7
BinName=BinNameCassette
NUps=0,2,4,9,16
;; Include a gap between pages in nUp mode
nUpGutter=1
;Media=1,400,427,451,461,462
Media=1,461,451,427,462
MediaType=1
UnsharpMask=0
Lightness=0
Contrast=0
Saturation=0
Aspect1=1
Data1=0
Dither=0
EEDumpLine=0
PlaneBuffer=1
Color=2
PixAlignX=32
PixAlignY=0
offsetX=120
offsetY=120
ZJS=1
PlaneMode=1
GCR=40
IcmFileKeys=5
RotateAble=0
;;SetupDLL=zvsetup,Setup
AsyncBuffer=16384
AsyncBlock=512
;blocking=512
CopyAble=1
PrintTicketNamespace=http://schemas.marvell.com/windows/2003/08/printing/xps2sd
ColorMatching=0
ZxBits=0x803D80F
;;uncomment the following to get 3-byte RGB data
BitsPixelExtra=8
Stream=ZJS
Compression=Zx
Compress=zdory.dll
ZxCodecBits=0x40200
BitonalBlocksize=40960
Data2=0xFCFD00
SourcePixel=1
DevicePixel=2
NetPage=callbackStubs
PageStats=1
CTASwitch=1
CTAMaxStripes=10
Borderless=4
;BorderlessX=4
;BorderlessY=4
;OversizeE=50
;OversizeM=127
OversizeE=10
OversizeM=25
PosterOverlap=10
CompressionQuality=95
CTAMaxPageSize=11718
OrderSuppliesUrl=

GetSupportUrl=

;MarginEnglish=45,45,45,45
;MarginMetric=45,45,45,45
MarginEnglish=0,0,0,0
MarginMetric=0,0,0,0
Fields=1,2,9,10,11,12,16
;Papers=1,5,6,7,9,11,70,268,269,270,271,272,273,274,37,20,27,43,275,276
Papers=1,9
;MinExtent=100,100
;MaxExtent=850,3000
MinExtent=100,40
MaxExtent=875,7500
MaxCopies=32767
PrintRate=60
UIUseDynamicMediaType=1
UIMediaSource=0
CustomDirLocation=1
ProfileBrand=AstroM1C
# define the default paper size shown for the printer
# e.g use 4x6
#DefaultPaper = 268

;
; Service tab buttons         TRANSLATE THE LABELS ServiceLabelxx
;TRANSLATE THIS SECTION
ServiceLabelL1=Print Con&figuration Page
ServiceCommandL1=config/ipage_config
ServiceHelpL1=Print_Configuration

ServiceLabelL2=데모 페이지 인쇄
ServiceCommandL2=config/ipage_colorbars
ServiceHelpL2=Print_Colorbars

ServiceLabelL3=구성 인쇄
ServiceCommandL3=config/ipage_diag
ServiceHelpL3=Print_Diagnostic_Page

;ServiceLabelL6=Printhead &Release
;ServiceCommandL6=config/sdk_ph_release
;ServiceHelpL6=Printhead_Release

;ServiceLabelR1=&Wipe Printhead
;ServiceCommandR1=config/sdk_wipe_head
;ServiceHelpR1=Wipe_Printhead

;ServiceLabelR6=System &Deprime
;ServiceCommandR6=config/sdk_system_deprime
;ServiceHelpR6=System_Deprime


ServiceLabelR1=&Quick Clean Printhead
ServiceCommandR1=config/sdk_ids_prime_level_1
ServiceHelpR1=Maintenance_Level_1

ServiceLabelR2=Nor&mal Clean Printhead
ServiceCommandR2=config/sdk_ids_prime_level_2
ServiceHelpR2=Maintenance_Level_2

ServiceLabelR3=Fu&ll Clean Printhead
ServiceCommandR3=config/sdk_ids_prime_level_3
ServiceHelpR3=Maintenance_Level_3

ServiceLabelR4=&Wipe Printhead
ServiceCommandR4=config/sdk_wipe_head
ServiceHelpR4=Wipe_Printhead

# uncomment the following section if a dEfault paper size needs
# to be defined per country
# e.g. AU and US defined to 4x6
#[DefaultPaper]
#61 = 268
#1 = 268

;; Settings for XPS printer
[MC Series Driver XPS to Zx]

;; Settings for OEM Generic printer
[MC Series Driver]
PrintProcessor=ZPP_AstroMCSeries
DataType=RAW
;;BitFlags=0x31041A
;; change to force all page to be color for avoiding momochrome in stitched jobs
BitFlags=0x31241A

[XPS options]
;; Values are: (JPEG = 2, PNG = 3, HDPHOTO = 4, TIFF = 5)
;; maximum limit is 8 formats
PassThru=2       ;; enables JPEG and PNG for XPS

[ICMFile]
MC Series Driver XPS to Zx=600.ICM
MC Series Driver=600.ICM

[BinNameCassette]
;TRANSLATE THIS SECTION
4 = 후면 급지대
7 = 기본 용지함

[PapersPerBin]
;4 = 1,5,6,7,9,11,70,268,269,270,271,272,273,274,37,20,27,43,275,276
;7 = 1,5,6,7,9,11,70,268,269,270,271,272,273,274,37,20,27,43,275,276
4 = 1,9
7 = 1,9

[MediaPerBin]
2 = 1,2
3 = 1,259,261

[PaperName]
;TRANSLATE THIS SECTION
1 = Letter 8 1/2 x 11in
;5 = Legal 8 1/2 x 14 in
;6 = Statement 5 1/2 x 8 1/2 in
;7 = Executive 7 1/4 x 10 1/2 in
9 = A4 210 x 297mm
;11 = A5 148 x 210 mm
;20 = Env. Com10 4 1/8 x 9 1/2 in
;27 = Env. DL 110 x 220 mm
;37 = Env. Monarch 3 7/8 x 7 1/2 in
;43 = Hagaki 100 x 148 mm
;70 = A6 105 x 148 mm
;268 = 4 x 6 in
;269 = 5 x 7 in
;270 = 5 x 8 in
;271 = 4 x 10 in
;272 = 4 x 11 in
;273 = 4 x 12 in
;274 = 8 x 10 in
;275 = 100 x 150 mm
;276 = 6 x 4 in

[PaperSize]
;43 = 1000,1480,2
;70 = 1050,1480,2
;268 = 400,600,4
;269 = 500,700,4
;270 = 500,800,4
;271 = 400,1000,4
;272 = 400,1100,4
;273 = 400,1200,4
;274 = 800,1000,4
;275 = 1000,1500,2
;276 = 600,400,4

[MediaName]
;TRANSLATE THIS SECTION
;1   = Default

;400 = Plain Paper
1 = 일반 용지
461 = Coated Paper
462 = Premium Glossy Label
427 = Glossy Label
451 = Matte Label

[MediaProfile]
; Format: Paper ID = Profile base name
;400 = Plain Paper
1 = Plain Paper
461 = Mitsubishi 9084
462 = Premium Glossy Label
427 = Glossy Label
451 = Matte Coated Label

[NUpName]
;TRANSLATE THIS SECTION
0  = 해제
2  = 2
4  = 4
6  = 6
9  = 9
16 = 16

[ColourProfile]
;TRANSLATE THIS SECTION
;Default=Default
