[Installation]
Product=S Series Driver
Configuration=ZSU_AstroSSeries.DLL
Driver=ZSD_AstroSSeries.DLL
UI=ZSU_AstroSSeries.DLL

[Units]
MarginPerInch=600
MarginPerCM=254     ; 300/2.54
ExtentPerInch=100

[DefaultPrinter]
DefaultFeed=1
;; Sets the print quality of the bitonal later
;;BitonalPrintQuality=800
PrintQuality=800
;; Set these values if additional resolutions are to be added
Resolution=800
;ResolutionXY=800,800, 1600,1600
;; These values specify the resolution the printer is capable
;; of printing at. By contrast, the PrintQuality value is what
;; we render at.
PhysicalResolutionX=1600
PhysicalResolutionY=1600
Capabilities=1,2,3,4,7,9,10,11,12,16
Formats=0,1,2,3,4,5,6
Bins=7,4
Source=7
BinName=BinNameCassette
NUps=0,2,4,9,16
;; Include a gap between pages in nUp mode
nUpGutter=1
Media=1,460,462,464,466,468,470
MediaType=1
UnsharpMask=0
Lightness=0
Contrast=0
Saturation=0
Aspect1=1
Data1=0
Dither=0
EEDumpLine=0
PlaneBuffer=1
Color=2
;PixAlignX=32
;rk - updated rounding
PixAlignX=16
PixAlignY=0
offsetX=120
offsetY=120
ZJS=1
PlaneMode=1
GCR=40
IcmFileKeys=5
RotateAble=0
;;SetupDLL=zvsetup,Setup
AsyncBuffer=16384
AsyncBlock=512
;blocking=512
CopyAble=1
PrintTicketNamespace=http://schemas.marvell.com/windows/2003/08/printing/xps2sd
ColorMatching=0
ZxBits=0x803D80F
;;uncomment the following to get 3-byte RGB data
BitsPixelExtra=8
Stream=ZJS
Compression=Zx
Compress=zdory.dll
ZxCodecBits=0x40200
BitonalBlocksize=40960
Data2=0xFCFD00
SourcePixel=1
DevicePixel=2
NetPage=callbackStubs
PageStats=1
CTASwitch=1
CTAMaxStripes=10
;Borderless=4
;rk - update to appx 3mm growth over 8.5in
Borderless=12
;BorderlessX=4
;BorderlessY=4
;OversizeE=50
;OversizeM=127
OversizeE=13
OversizeM=30
PosterOverlap=10
CompressionQuality=95
CTAMaxPageSize=11718
InkTypeSet=1
OrderSuppliesUrl=



GetSupportUrl=



;MarginEnglish=45,45,45,45
;MarginMetric=45,45,45,45
MarginEnglish=0,0,0,0
MarginMetric=0,0,0,0
Fields=1,2,3,4,9,10,11,12,16
;Papers=1,5,6,7,9,11,70,268,269,270,271,272,273,274,37,20,27,43,275
Papers=1,5,6,7,9,11,70,13,14,268,269,270,271,272,273,274,275,37,281,19,276,20,277,27,278,28,279,35,280,43,282,283,284
;MinExtent=300,325
;MaxExtent=950,3000
MinExtent=100,300
MaxExtent=877,4000
MaxCopies=32767
PrintRate=60
UIUseDynamicMediaType=1
UIMediaSource=0
#UIBooklet=0
#UIDuplex=1
CustomDirLocation=1
ProfileBrand=AstroS
# define the default paper size shown for the printer
# e.g use 4x6
#DefaultPaper = 268

;
; Service tab buttons         TRANSLATE THE LABELS ServiceLabelxx
;TRANSLATE THIS SECTION
ServiceLabelL1=Imprimer page config
ServiceCommandL1=config/ipage_config
ServiceHelpL1=Print_Configuration

ServiceLabelL2=Imprimer page histogramme
ServiceCommandL2=config/ipage_colorbars
ServiceHelpL2=Print_Colorbars

ServiceLabelL3=Imprimer page diagnostic
ServiceCommandL3=config/ipage_diag
ServiceHelpL3=Print_Diagnostic_Page

; dja removed in R12
;ServiceLabelL6=Printhead &Release
;ServiceCommandL6=config/sdk_ph_release
;ServiceHelpL6=Printhead_Release

ServiceLabelR1=Nettoyage rapide tête
ServiceCommandR1=config/sdk_ids_prime_level_1
ServiceHelpR1=Maintenance_Level_1

ServiceLabelR2=Nettoyage normal tête
ServiceCommandR2=config/sdk_ids_prime_level_2
ServiceHelpR2=Maintenance_Level_2

ServiceLabelR3=Nettoyage complet tête
ServiceCommandR3=config/sdk_ids_prime_level_3
ServiceHelpR3=Maintenance_Level_3

ServiceLabelR4=Essuyer tête d'impr
ServiceCommandR4=config/sdk_wipe_head
ServiceHelpR4=Wipe_Printhead

; dja removed in R12
;ServiceLabelR6=System &Deprime
;ServiceCommandR6=config/sdk_system_deprime
;ServiceHelpR6=System_Deprime

# uncomment the following section if a dEfault paper size needs
# to be defined per country
# e.g. AU and US defined to 4x6
#[DefaultPaper]
#61 = 268
#1 = 268

;; Settings for XPS printer
[S Series Driver XPS to Zx]

;; Settings for OEM Generic printer
[S Series Driver]
PrintProcessor=ZPP_AstroSSeries
DataType=RAW
;;BitFlags=0x31041A
;; change to force all page to be color for avoiding momochrome in stitched jobs
BitFlags=0x31241A

[XPS options]
;; Values are: (JPEG = 2, PNG = 3, HDPHOTO = 4, TIFF = 5)
;; maximum limit is 8 formats
PassThru=2       ;; enables JPEG and PNG for XPS

[ICMFile]
S Series Driver XPS to Zx=600.ICM
S Series Driver=600.ICM

[BinNameCassette]
;TRANSLATE THIS SECTION
4 = Bac d'alimentation manuelle

7 = Bac principal


[PapersPerBin]
4 = 1,5,6,7,9,11,70,13,14,268,269,270,271,272,273,274,275,37,281,19,276,20,277,27,278,28,279,35,280,43,282,283,284
7 = 1,5,6,7,9,11,70,13,14,268,269,270,271,272,273,274,275,37,281,19,276,20,277,27,278,28,279,35,280,43,282,283,284

[MediaPerBin]
2 = 1,2
3 = 1,259,261

[PaperName]
;TRANSLATE THIS SECTION
1 = Lettre 8 1/2 x 11 pouces
5 = Legal 8 1/2 x 14 pouces
6 = Déclaration 5 1/2 x 8 1/2 pouces
7 = Executive 7 1/4 x 10 1/2 pouces
9 = A4 210 x 297 mm
11 = A5 148 x 210 mm
13 = B5 (JIS) 182 x 257 mm
14 = Folio 8 1/2 x 13 pouces
19 = Env. Com9 3 7/8 x 8 7/8 pouces - Portrait
20 = Env. Com10 4 1/8 x 9 1/2 pouces - Portrait
27 = Env. DL 110 x 220 mm - Portrait
28 = Env. C5 162 x 229 mm - Portrait
35 = Env. B5 176 x 250 mm - Portrait
37 = Env. Monarch 3 7/8 x 7 1/2 pouces - Portrait
43 = Hagaki 100 x 148 mm - Portrait
70 = A6 105 x 148 mm
268 = 4 x 6 pouces
269 = 5 x 7 pouces
270 = 5 x 8 pouces
271 = 4 x 10 pouces
272 = 4 x 11 pouces
273 = 4 x 12 pouces
274 = 8 x 10 pouces
275 = 100 x 150 mm
276 = Env. Com9 3 7/8 x 8 7/8 pouces - Paysage
277 = Env. Com10 4 1/8 x 9 1/2 pouces - Paysage
278 = Env. DL 110 x 220 mm - Paysage
279 = Env. C5 162 x 229 mm - Paysage
280 = Env. B5 176 x 250 mm - Paysage
281 = Env. Monarch 3 7/8 x 7 1/2 pouces - Paysage
282 = Hagaki 100 x 148 mm - Paysage
283 = 6 x 9 pouces - Portrait
284 = 6 x 9 pouces - Paysage

[PaperSize]
35 = 1760,2500,2
43 = 1000,1480,2
70 = 1050,1480,2
268 = 400,600,4
269 = 500,700,4
270 = 500,800,4
271 = 400,1000,4
272 = 400,1100,4
273 = 400,1200,4
274 = 800,1000,4
275 = 1000,1500,2
;276 = 850,388,4
;277 = 850,413,4
276 = 877,388,4
277 = 877,413,4
;278 = 2150,1100,2
;279 = 2150,1620,2
;280 = 2150,1760,2
278 = 2200,1100,2
279 = 2227,1620,2
280 = 2227,1760,2
281 = 750,388,4
282 = 1480,1000,2
283 = 600,900,4
;284 = 850,600,4
284 = 877,600,4

[MediaName]
;TRANSLATE THIS SECTION
;1   = Default
1 = Papier ordinaire
460 = Papier couché mat
462 = Papier brillant Premium
464 = Étiquette en papier brillant
466 = Étiquette en papier couché mat
468 = Premium Envelope
470 = Brown Corrugated Paper

[MediaProfile]
;TRANSLATE THIS SECTION
; Format: Paper ID = Profile base name
1 = Plain Paper
460 = Matte Coated Paper
462 = Premium Glossy Label
464 = Glossy Label
466 = Matte Coated Label
468 = Lindenmayer 220
470 = Lindenmayer 220

[NUpName]
;TRANSLATE THIS SECTION
0  = Désactivation (1-Up)
2  = 2-Up
4  = 4-Up
6  = 6-Up
9  = 9-Up
16 = 16-Up

[ColourProfile]
;TRANSLATE THIS SECTION
;Default=Default
